|  |  |
| --- | --- |
| HEATED FORCEPS | TICK REQUIREMENTS |
| 1. Dimensions +/- 200 x 200 x 100mm
 |  |
| 1. Quick heating
 |  |
| 1. Variable temperature control
 |  |
| 1. Small tips of 1 – 2 mm
 |  |
| 1. Voltage 220V/50Hz
 |  |
| 1. Temperature range 30 to 80 degrees Celsius
 |  |
| 1. Instruction manual
 |  |
| 1. Manufacturer’s warranty
 |  |
| 1. At least two forceps
 |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
| Lab Manager Name: |  |
| Lab Manager Signature: |  |
| Date: |  |
| QAC Name: |  |
| QAC Signature: |  |
| Date: |  |